**DUNBAR HEAT SHRINKABLE TUBING**

Part Number Cross Reference

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Dunbar Part No.** | **AS23053/** | **UL-VW-1** | **TE/Raychem** | **Sumitomo** | **3M** | **Canusa** | **Alpha** |

**Polyolefin Tubing**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Dunbar-1605**  2:1 -Flexible -105•C, 600V – UL rated |  | Yes |  | C2 A4 |  | CPX-51 |  |
| **Dunbar-1625**  2:1- Flexible - 125•C,600V, UL&CSA |  | Yes |  | F2, F32  F2(Z) | CP-221 |  | FIT-221V |
| **Dunbar-1635F**  2:1 Flexible, - 135•C,600V, UL&CSA & AS23053/5 | /5  Class 1,2,3 | Yes | RNF—100  Versafit | SM12, B2  A2, SM35 | FP-301  FP-301VW | CPX100  P0135  CPX876 | FIT-221  FIT-221B |
| **Dunbar-1635F Y/G**  2:1 Flexible - 135•C,600V |  | Yes | DCPT | B2 (Y/G) |  | CPX201 | FIT-260 |
| **Dunbar-1625GT**  2:1 Very Flexible, 125•C,150V, thin wall, UL & CSA rated |  | Yes | Versafit V4 | F$(TW) |  | None | FIT-221-TW |
| **DUNBAR-1635S**  2:1 Semi Rigid, 135•C,600V  Rating AS23053/6\* Pending QPL | /6\*  Class 1 & 2  Pending QPL | Yes | CRN | B8  D | SR-350 | CHM-140  HM-140 | FIT-295 |
| **Dunbar-3535**  3:1 Flexible, 135•C,600V, UL& CSA,  AS23053/5\* Pending QPL | /5\*  Class 4  \*Pending QPL | Yes | RNF-3000 | SM23  B2 (3X)  A2 (3X) | SFTW-203 | CPX300 | FIT-321V |
| **Dunbar-4365**  4:1 Flexible, 135•C,600V, UL & CSA |  | Yes | RP-4800 | B2 (4X) |  | None | FIT-421 |



**Specialty Tubing**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Dunbar Part No.** | **AS23053/** | **UL-VW-1** | **TE/Raychem** | **Sumitomo** | **3M** | **Canusa** | **Alpha** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Dunbar-CRCFR**  2:1 120•C rating, AS23053/1 | /1  Class 1 & 2 | Yes | NT-FR  NT | R10 | NST | CNP 200 | FIT-600 |
| **Dunbar-1675**  2:1 175•C, 600V, UL &AS23053/8 | /8 | Yes | Kynar  RW-175 | K | Kynar | CKN 175  HA 150 | FIT-350 |
| **Dunbar-3675**  3:1 175•C, 600V, UL |  | Yes |  |  |  |  |  |
| **Dunbar-DRET**  2:1, 175•C, 600V, | Discontinued use DR150 | Yes | DR-25 | R120 |  | CDR 625 | None |
| **Dunbar-DR150**  2:1, 150•C, 600V, AS23053/16 | /16 | Yes | DR-25 | R120 |  | CDR 625 | None |
| **Dunbar-FK150**  2:1, 200•C, 600V | /13 | Yes | Viton | KH230  SM60  SM3-60 | VTN-200 | Deray Vt 220 |  |

**Dual Wall, Polyolefin Tubing**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Dunbar Part No.** | **AS23053/** | **UL-VW-1** | **TE/Raychem** | **Sumitomo** | **3M** | **Canusa** | **Alpha** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Dunbar-2960NW**  3:2 Flexible, 90°- Semi Rigid |  | N/A |  | 02 |  |  |  |
| **Dunbar-1625W**  2:1 Flexible, 125°, 600V, UL/CSA, AS233053/4 | /4  Class 2 | N/A | TAT-125 | O2B2  O2C  SM24 | EPS-200 |  | FIT-750 |
| **Dunbar-3625WS**  3:1 Semi Rigid, 135°, 600V, AS233053/4 | /4  Class 1 | N/A | SCL | W5DL | MW |  | FIT-309 |
| **Dunbar-3535W**  3:1 flexible, 135°, 600V, AS233053/4 | /4  Class 3 | N/A | ATUM-3:1  DWP-125 | W3B2  W3F2  W3C | EPS-300 | CPA300  CPA100  (CPA100 NOT UL) | FIT-321 |
| **Dunbar-4635W**  4:1 Flexible, 135°, 600V, |  | N/A | ATUM-4:1 |  | EPS-400 |  | None |
| **Dunbar-4635WS**  4:1 Semi Rigid, 135°, 600V, |  | N/A | ES-2000  ES-1000 | SA2F | SMS  TES | Splicemelt | None |
| **Dunbar-4365WT**  4:1 Flexible, 135°, Thin Wall, |  | N/A | ATUM-4:1 | W3B2(4X) | EPS-400 |  |  |
| **Dunbar-4650WS**  4:1 Semi Rigid, 150°, 600V,  Fully Flame Retardant |  | N/A | FL 2500  SCT | None |  | CFRA | None |

**Medium & Heavy Wall Tubing**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Dunbar Part No. | AS23053/ | UL-VW-1 | TE/Raychem | Sumitomo | 3M | Canusa | Alpha |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Dunbar-CATV**  3:1, Flexible, Adhesive Lined, Medium Wall, 125°C, 600V |  | N/A | TCS  SCTV |  | CCT | CFTV |  |
| **Dunbar-CMWT**  3:1, Semi Rigid, Adhesive Lined, Medium Wall, 125°C, 600V |  | N/A | RMW  SST  BSTS |  |  | CFM | FIT-700 |
| **Dunbar-PMWT-FR**  3:1, Semi Rigid, AS23053/15, C1 & C2, ABS, DNV | /15  C1 & C2 | N/A | SST-FR  BSTS-FR |  | MDT |  |  |
| **Dunbar-CHWT**  3:1, Semi Rigid, Adhesive Lined, Heavy Wall, 125°C, 600V |  | N/A | RHW  SST  BSTS |  |  | CFW |  |
| **Dunbar-PHWT-FR**  3:1, Semi Rigid, AS23053/15 C1 & C2  ABS &DNV | /15  C1 & C2 | N/A | SST-FR  BSTS-FR  HF |  | HDT | FCFW |  |
| **Dunbar-BBLV**  3:1, Adhesive Lined, Medium Wall, 125°C, 1kV |  | N/A |  |  |  |  |  |
| **Dunbar-BBHV**  3:1, Adhesive Lined, Medium Wall, 125°C, 25kV |  | N/A |  |  |  |  |  |
| **Dunbar-BBHT**  3:1, Adhesive Lined, Medium Wall, 125°C, 35kV |  | N/A |  |  |  |  |  |

**Non-Shrinkable Tubing**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Dunbar Part No. | AS23053/ | UL-VW-1 | TE/Raychem | Sumitomo | 3M | Canusa | Alpha |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Dunbar-EIT-600**  125°C, 600V, UL & CSA Rated |  | **Yes** |  |  |  |  |  |