**DUNBAR HEAT SHRINKABLE TUBING**

Part Number Cross Reference

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Dunbar Part No.**  | **AS23053/** | **UL-VW-1** | **TE/Raychem** | **Sumitomo** | **3M** | **Canusa** | **Alpha** |

**Polyolefin Tubing**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Dunbar-1605**2:1 -Flexible -105•C, 600V – UL rated  |  | Yes |  | C2 A4 |  | CPX-51 |  |
| **Dunbar-1625**2:1- Flexible - 125•C,600V, UL&CSA  |  | Yes |  | F2, F32F2(Z) | CP-221 |  | FIT-221V |
| **Dunbar-1635F**2:1 Flexible, - 135•C,600V, UL&CSA & AS23053/5 | /5Class 1,2,3 | Yes | RNF—100Versafit | SM12, B2A2, SM35 | FP-301FP-301VW | CPX100P0135CPX876 | FIT-221FIT-221B |
| **Dunbar-1635F Y/G**2:1 Flexible - 135•C,600V |  | Yes | DCPT | B2 (Y/G) |  | CPX201 | FIT-260 |
| **Dunbar-1625GT**2:1 Very Flexible, 125•C,150V, thin wall, UL & CSA rated  |  | Yes | Versafit V4 | F$(TW) |  | None | FIT-221-TW |
| **DUNBAR-1635S**2:1 Semi Rigid, 135•C,600V Rating AS23053/6\* Pending QPL | /6\*Class 1 & 2 Pending QPL | Yes | CRN | B8D | SR-350 | CHM-140HM-140 | FIT-295 |
| **Dunbar-3535** 3:1 Flexible, 135•C,600V, UL& CSA, AS23053/5\* Pending QPL  | /5\*Class 4\*Pending QPL | Yes | RNF-3000 | SM23B2 (3X)A2 (3X) | SFTW-203 | CPX300 | FIT-321V |
| **Dunbar-4365**4:1 Flexible, 135•C,600V, UL & CSA  |  | Yes | RP-4800 | B2 (4X) |  | None | FIT-421 |



**Specialty Tubing**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Dunbar Part No.**  | **AS23053/** | **UL-VW-1** | **TE/Raychem** | **Sumitomo** | **3M** | **Canusa** | **Alpha** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Dunbar-CRCFR**2:1 120•C rating, AS23053/1 | /1Class 1 & 2 | Yes | NT-FRNT | R10 | NST | CNP 200 | FIT-600 |
| **Dunbar-1675**2:1 175•C, 600V, UL &AS23053/8 | /8 | Yes | KynarRW-175 | K | Kynar | CKN 175HA 150 | FIT-350 |
| **Dunbar-3675**3:1 175•C, 600V, UL  |  | Yes |  |  |  |  |  |
| **Dunbar-DRET**2:1, 175•C, 600V,  | Discontinued use DR150 | Yes | DR-25 | R120 |  | CDR 625 | None |
| **Dunbar-DR150**2:1, 150•C, 600V, AS23053/16 | /16 | Yes | DR-25 | R120 |  | CDR 625 | None |
| **Dunbar-FK150**2:1, 200•C, 600V | /13 | Yes | Viton | KH230SM60SM3-60 | VTN-200 | Deray Vt 220 |  |

**Dual Wall, Polyolefin Tubing**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Dunbar Part No.**  | **AS23053/** | **UL-VW-1** | **TE/Raychem** | **Sumitomo** | **3M** | **Canusa** | **Alpha** |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Dunbar-2960NW**3:2 Flexible, 90°- Semi Rigid  |  | N/A |  | 02 |  |  |  |
| **Dunbar-1625W**2:1 Flexible, 125°, 600V, UL/CSA, AS233053/4 | /4 Class 2 | N/A | TAT-125 | O2B2O2CSM24 | EPS-200 |  | FIT-750 |
| **Dunbar-3625WS** 3:1 Semi Rigid, 135°, 600V, AS233053/4 | /4 Class 1 | N/A | SCL | W5DL | MW |  | FIT-309 |
| **Dunbar-3535W**3:1 flexible, 135°, 600V, AS233053/4 | /4 Class 3 | N/A | ATUM-3:1DWP-125 | W3B2W3F2W3C | EPS-300 | CPA300CPA100(CPA100 NOT UL) | FIT-321 |
| **Dunbar-4635W**4:1 Flexible, 135°, 600V,  |  | N/A | ATUM-4:1 |  | EPS-400 |  | None |
| **Dunbar-4635WS**4:1 Semi Rigid, 135°, 600V,  |  | N/A | ES-2000ES-1000 | SA2F | SMSTES | Splicemelt  | None |
| **Dunbar-4365WT**4:1 Flexible, 135°, Thin Wall,  |  | N/A | ATUM-4:1 | W3B2(4X) | EPS-400 |  |  |
| **Dunbar-4650WS**4:1 Semi Rigid, 150°, 600V, Fully Flame Retardant  |  | N/A | FL 2500SCT | None |  | CFRA | None |

**Medium & Heavy Wall Tubing**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Dunbar Part No.  | AS23053/ | UL-VW-1 | TE/Raychem | Sumitomo | 3M | Canusa | Alpha |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Dunbar-CATV**3:1, Flexible, Adhesive Lined, Medium Wall, 125°C, 600V |  | N/A | TCSSCTV |  | CCT | CFTV |  |
| **Dunbar-CMWT**3:1, Semi Rigid, Adhesive Lined, Medium Wall, 125°C, 600V |  | N/A | RMWSSTBSTS |  |  | CFM | FIT-700 |
| **Dunbar-PMWT-FR**3:1, Semi Rigid, AS23053/15, C1 & C2, ABS, DNV | /15C1 & C2 | N/A | SST-FRBSTS-FR |  | MDT |  |  |
| **Dunbar-CHWT**3:1, Semi Rigid, Adhesive Lined, Heavy Wall, 125°C, 600V |  | N/A | RHWSSTBSTS |  |  | CFW |  |
| **Dunbar-PHWT-FR**3:1, Semi Rigid, AS23053/15 C1 & C2ABS &DNV | /15C1 & C2 | N/A | SST-FRBSTS-FRHF |  | HDT | FCFW |  |
| **Dunbar-BBLV**3:1, Adhesive Lined, Medium Wall, 125°C, 1kV |  | N/A |  |  |  |  |  |
| **Dunbar-BBHV**3:1, Adhesive Lined, Medium Wall, 125°C, 25kV |  | N/A |  |  |  |  |  |
| **Dunbar-BBHT**3:1, Adhesive Lined, Medium Wall, 125°C, 35kV |  | N/A |  |  |  |  |  |

**Non-Shrinkable Tubing**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Dunbar Part No.  | AS23053/ | UL-VW-1 | TE/Raychem | Sumitomo | 3M | Canusa | Alpha |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Dunbar-EIT-600**125°C, 600V, UL & CSA Rated  |  | **Yes** |  |  |  |  |  |